Controller: #9 Imagine 128 Series 2 Memory Configurations: 4MB EDO VRAM fixed Horizontal Sync Signals: 31.5KHz - 100KHz Vertical Refresh: 60Hz - 150 Hz Maximum Dot Clock: 220MHz (250MHz for 8 Megabyte card) Video Output Signal: Analog Video Connector: Standard 15-pin D-shell Feature Connector: VESA 26-pin header 32-Bit Bus Architecture: PCI Local Bus Approvals: VESA DPMS & Energy Star Compliant, FCC Class B Certified, CE Mark, TUV Monitors Supported: Standard and multi-frequency analog monitors Drivers Supported: Microsoft Windows 3.1x, Windows 95 ,Windows NT v3.51 (3D-DDI), Windows NT 4.0, OS/2, AutoCAD 95/NT, MicroStation 95/NT, Open-GL

Download Adobe Print Document Format version(s) of the DataSheet:

English Spanish French Italian

i2enpdf.pdf i2sppdf.pdf i2frpdf.pdf i2itpdf.pdf

Download the Adobe Acrobat PDF Viewer

Features | Performance Data | Tech Specs | Why We Built It | HawkEye | Number Nine Home